## Analog Video Crossbar

The WDM-based Analog Video Crossbar filter can select or route analog video. The single output stream represents a hardware path for analog baseband video. One of the input pins comes from a TV Tuner (the TV Tuner Filter). Other input pins support video streams.

The Analog Video Crossbar filter exposes the IAMCrossbar interface, which is used for routine source selection.

This filter is available through Windows 98 and Windows NT 5.

© 1997 Microsoft Corporation. All rights reserved. Terms of Use.