## TV Tuner

The TV Tuner filter selects an analog broadcast or cable channel to be viewed. The single output stream is a hardware path for analog baseband video. This output should be an input to the Analog Video Crossbar filter. The input pins include an input for cable and an antenna input.

The TV Tuner filter exposes the IAMTVTuner interface, which is used for channel selection.

This filter is available through the Windows 98 and Windows NT 5.

© 1997 Microsoft Corporation. All rights reserved. Terms of Use.