## V

VITC
  Vertical Interval Timecode. Timecode information stored in a video signal's vertical blanking interval. It is usually located on one or two lines somewhere between lines 10 and 20.
vertical blanking interval
  A synchronizing period in the video signal when no active picture information is transmitted.
VPE
  Video port extensions. Extensions to the DirectDraw API to control the video stream from the video port, within the context of VGA memory.
VTR
  Video tape recorder.

© 1997 Microsoft Corporation. All rights reserved. Terms of Use.