## I

input pin
  A pin that accepts data into the filter.
interlace
  Raster scan involving frames that are composed of two fields. See also bob and weave.
interleaving
  The arrangement of corresponding video frames and audio samples in a file. Typically, one or more frames of video data are intermixed in the file with a certain number of samples of audio data. The data sequence is audio, followed by video, followed by audio, followed by video, and so on, rather than all audio data followed by all video data. The way a file is interleaved affects playback efficiency and the ability to stream the file.

© 1997 Microsoft Corporation. All rights reserved. Terms of Use.