## DV Muxer

The DV Muxer filter multiplexes compressed DV video with compressed DV audio.

The DV Muxer filter accepts the following input media types:

From the video input pin:

MEDIATYPE_Video
MEDIASUBTYPE_dvsd/dvhd/dvsl
FORMAT: VIDEOINFO

From the audio input pin:

MEDIATYPE_Audio
MEDIASUBTYPE_wave
FORMAT: WAVEFORMATEX/NULL

The DV Muxer filter sends the following output media type:

From the video output pin:

MEDIATYPE_Interleaved(iavs)
MEDIASUBTYPE_dvsd/dvhd/dvsl
FORMAT: DVINFO

To see a diagram of how to use the DV Muxer filter with the DV Video Encoder filter, see DV Video Encoder.

© 1997 Microsoft Corporation. All rights reserved. Terms of Use.